**Table of Contents**

[1. Overview 2](#_Toc131837858)

[1.1. Workflow 2](#_Toc131837859)

## Workflow

Diagram

Description automatically generated with low confidence

## CAN bus command data structure.

|  |  |  |  |
| --- | --- | --- | --- |
| **Commands** | **CMD** | **Direction** | **Description** |
| CAN\_ID\_BL\_APP\_ERASE | 0x0CFFD000 | APP 🡪 MCU |  |
| CAN\_ID\_BL\_APP\_ERASE\_APOS | 0x0CFFD001 | MCU 🡪 APP |  |
| CAN\_ID\_BL\_APP\_ERASE\_ANEG | 0x0CFFD002 | MCU 🡪 APP |  |
| CAN\_ID\_BL\_STOP | 0x0CFFD003 | APP 🡪 MCU |  |
| CAN\_ID\_BL\_STOP\_APOS | 0x0CFFD004 | MCU 🡪 APP |  |
| CAN\_ID\_BL\_STOP\_ANEG | 0x0CFFD005 | MCU 🡪 APP |  |
| CAN\_ID\_BL\_CPU\_RESET | 0x0CFFD006 | APP 🡪 MCU |  |
| CAN\_ID\_BL\_CPU\_RESET\_APOS | 0x0CFFD007 | MCU 🡪 APP |  |
| CAN\_ID\_BL\_VER\_REQ | 0x0CFFD008 | APP 🡪 MCU |  |
| CAN\_ID\_BL\_VER\_REQ\_RSP | 0x0CFFD009 | MCU 🡪 APP |  |
| CAN\_ID\_BL\_MAP\_REQ | 0x0CFFD00A | APP 🡪 MCU |  |
| CAN\_ID\_BL\_MAP\_REQ\_RSP\_ARM | 0x0CFFD00B | MCU 🡪 APP |  |
| CAN\_ID\_BL\_MAP\_REQ\_RSP\_C2K | 0x0CFFD00C | MCU 🡪 APP |  |
| CAN\_ID\_BL\_ADDR | 0x0CFFD020 | APP 🡪 MCU |  |
| CAN\_ID\_BL\_ADDR\_APOS | 0x0CFFD021 | MCU 🡪 APP |  |
| CAN\_ID\_BL\_ADDR\_ANEG | 0x0CFFD022 | MCU 🡪 APP |  |
| CAN\_ID\_BL\_DATA | 0x0CFFD023 | APP 🡪 MCU |  |
| CAN\_ID\_BL\_DATA\_APOS | 0x0CFFD024 | MCU 🡪 APP |  |
| CAN\_ID\_BL\_DATA\_ANEG | 0x0CFFD025 | MCU 🡪 APP |  |

### Packet CAN\_ID\_BL\_APP\_ERASE